A Codes
FUNCTION	SEL	CODE	FUNCTION	SEL	CODE	
Repeater Enable	4100 	A_ _	Reverse Patch enable	4110	A_ _	
Repeater Disable	4100 	A_ _	Reverse Patch disable	4111	A_ _	
Repeater PL Access	4102 	A_ _	Master Enable	4112	A_ _	
Repeater Carrier (PL off)	4103 	A_ _	Master disable	4113	A_ _	
Auto-patch Enable	4104 	A_ _	Remote Base enable	4114	A_ _	
Auto-patch Disable	4105 	A_ _	Remote Base disable	4115	A_ _	
Patch PL Access	4106 	A_ _	Control Code disable	4116	A_ _	
Patch Carrier (PL off)	4106 	A_ _	Control code enable	4117	A_ _	
Answer Phone enable	4120 	A_ _	Dialing 911 enable/disable	4122	A_ _	
Answer Phone disable	4121 	A_ _	DTMF Access enable/disable	4133	A_ _	
Remote Base w/prt disabled	4124 	A_ _	Patch outside line digit	4130	0 _	

D Codes
FUNCTION	SEL	CODE	FUNCTION	SEL	CODE	
External ID enable/disable	4140	D_ _	Patch Long Dist enable	4150	D_ _	
Remote Base Beep	4141	D_ _	Patch Long Dist disable	4151	D_ _	
Dial 9 enable/disable	4142	D _ _
	Patch Timeout enable/disable	4152	D_ _	
CW ID Program	4143	D_ _@	Patch User Mute enable/disable	4153	D_ _	
DTMF Muting enable/disable	4144	D_ _	Patch Normal Timeout	4154	D_ _	
(not used)	4145	D_ _
	Patch timer reset on input	4155	D_ _	
Patch Pulse dial	4146	D_ _@	*up/#down Patch enable/disable	4156	D_ _@	
Patch DTMF dial	4147	D_ _@	Reverse Patch Signal enable/disable	4157	D_ _	
CW ID Continuous	4160	D_ _	Patch Duplex enable/disable	4170	D_ _	
AUX output	4162	D_ _
	Timeout enable/disable	4171	D_ _	
CW ID enable/disable	4163	D_ _	Programming disable	4172	D_ _ (D7A)	
Ext ID record	4164	D_ _	Programming enable 1	4173	D_ _ (D7B)	
CW Tail Beep Program	4165	D_ _	Programming enable 2	4174	D_ _ (D7C)	
CW Tail/Normal Beep	4166	D_ _	PL Control enable/disable	4167	D_ _	
Note: Codes with @ require programming enabled to function.
Note: Codes in parenthesis are default and activate when the controller is powered off

User Codes
FUNCTION	SEL	CODE	FUNCTION	SEL	CODE	
Remote Base On	4071	*_ _	Patch On	4070	*_ _	
Remote Base Off	4061	#_	Long Dist Patch On	4072	*_ _	
A Equivalent	4062	#_	Anti-Kerchunk On/Off	4073	*_ _	
D Equivalent	4063	#_	Patch Off	4066	#_	
Call In On	4064	#_	PL Override Code	4131	*_ _	
Patch Reset	4065	#_	DTMF Access Code	4132	*_ _	
Reverse Patch Signal	4067	#_	Autodial Prefix	4134	#_	
Force CW ID	4126	#_	Remote Base XMT ON/OFF	4125	#*	
Force External ID	4127	#_	DTMF Pad Tester	Fixed	#0 (fixed)	

Repeater Parameters
Note: All timer values are in hex, use a decimal to hex conversion calculator like XP has.
FUNCTION	SEL	Value	Default Value	Sample	
Repeater Timeout	4050	42@	12=3 minutes	11x60=660/10=66=42
	
Patch Timeout	4051	42@	12=3 minutes		
Repeater Tail Time	4052	28@	1*=3 seconds		
CW ID Speed	4053	_ _@	07=15		
CW ID Tone	4057	_ _@	02=500 Hz		
CW ID timer interval	4076	_ _@	3C=8 minutes	9x60=540/10=54=36	
Tail Beep Time	4054	_ _@	07=.7 seconds		
Tail Beep Program	4055	_ _ _ _@	1234=1000 500 330 250 Hz		
Number rings to answer	4077	_ _@	10=about one ring		
Invalid DTMF limit	4137	_ _@	255		
Note: Codes with @ require programming enabled to function.